Introduction to IT – 26.09.19

* CRT – Cathode Ray Tube – Uses electron gun for image rendering.
* LCD – Liquid Crystal Display – Just better for everything bar refresh rate
* Tactile – Touch
* USB – General purpose input output
* USB superior due to it’s general GPIO features, higher bandwidth and its inexpensive nature.
* USB is completely backwords compatible
* Power Supply – Converts AC power into DC power of the correct voltage
* HDD/SSD are **EXTERNAL** devices